
	Electrical Estimate
Residential and light commercial
	Estimate no. ____________________
Issued ____________  Expires ____________



JOB TYPE: COMPLETE ONLY THE LETTERED BLOCK THAT APPLIES
	☐   A.  Service call
	☐   B.  Panel upgrade
	☐   C.  Rewire



CONTRACTOR AND CUSTOMER
	BUSINESS NAME
	ELECTRICAL LICENSE NO.

	BUSINESS ADDRESS
	PHONE

	CUSTOMER NAME
	SERVICE ADDRESS

	BILLING ADDRESS, IF DIFFERENT
	CONTACT PHONE AND EMAIL



SITE CONDITIONS RECORDED AT THE WALKTHROUGH
	EXISTING SERVICE SIZE (AMPS)
	PANEL LOCATION

	PANEL MAKE AND TYPE
	METER NUMBER AND TYPE

	APPROXIMATE AGE OF WIRING
	WIRING TYPE OBSERVED

	ATTIC / CRAWLSPACE ACCESS
	KNOWN CODE OR SAFETY ISSUES



SCOPE OF WORK, IN PLAIN SENTENCES, BEFORE ANY PRICING:
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________

	A
	SERVICE CALL     diagnostic visit and repair



	TRIP OR DIAGNOSTIC FEE  $
	CREDITED AGAINST REPAIR?  YES / NO

	INCLUDED TIME
	HOURLY RATE AFTER INCLUDED TIME  $



	FINDING
	REPAIR RECOMMENDED
	PARTS
	AMOUNT

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



	If the fault proves larger than diagnosed, work stops and a revised estimate is issued before continuing. Nothing beyond the amount above is billed without written approval.



	B
	PANEL UPGRADE     service change, meter and mast



	EXISTING SERVICE (AMPS)
	NEW SERVICE (AMPS)

	NEW PANEL MAKE AND MODEL
	NUMBER OF SPACES

	METER WORK REQUIRED
	MAST / WEATHERHEAD WORK REQUIRED

	GROUNDING AND BONDING SCOPE
	SURGE PROTECTION INCLUDED?  YES / NO



BREAKER SCHEDULE
	CIRCUIT
	SERVES
	SIZE (A)
	TYPE (STD / AFCI / GFCI / DUAL)
	AMOUNT

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



UTILITY COORDINATION AND OUTAGE
	UTILITY COMPANY
	WHO CONTACTS THE UTILITY

	DISCONNECT / RECONNECT REQUIRED
	EXPECTED POWER-OFF WINDOW (HOURS)



	The outage window and the inspection slot are set by the utility and the authority having jurisdiction, not by the crew. Dates are held on acceptance and confirmed once the permit is issued.



	C
	REWIRE     phased, priced by area and access



	AREA OR ROOM
	CIRCUITS
	DEVICES
	FIXTURES
	ACCESS NOTES
	AMOUNT

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	



	PHASING (ORDER OF AREAS)
	OCCUPIED DURING WORK?  YES / NO

	TEMPORARY POWER ARRANGEMENT
	DRYWALL: CUT ONLY / PATCH / PATCH AND PAINT

	EXISTING WIRING REMOVED OR ABANDONED
	REMEDIATION REQUIRED (ALUMINUM, KNOB-AND-TUBE)



LABOR
	CLASSIFICATION
	HOURS
	RATE
	AMOUNT

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


Or flat price for the scope above, with included hours stated: $ ______________ for ________ hours.

MATERIALS AND ALLOWANCES
	ITEM
	QTY
	UNIT
	AMOUNT

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



ALLOWANCES
	ALLOWANCE ITEM
	AMOUNT HELD
	RECONCILIATION

	
	
	

	
	
	

	
	
	



Each allowance is a held amount, not a cap. The difference between the allowance and the actual cost of the item selected is billed or credited at cost.
☐  Customer-supplied fixtures. Labor is quoted on the basis that items arrive complete, undamaged and listed for the application. A return trip caused by a missing part or an incompatible fixture is billable at the service rate. Warranty on a customer-supplied item is the manufacturer’s; installation labor carries the contractor’s warranty.

PERMITS AND INSPECTIONS
	PERMIT OR INSPECTION
	AUTHORITY HAVING JURISDICTION
	PULLED BY
	FEE AT COST

	
	
	
	

	
	
	
	

	
	
	
	


Permit fees are listed at cost and are not marked up. Work does not close out until the required inspections pass. A failed inspection caused by customer-supplied equipment is billable.

EXCLUSIONS AND ASSUMPTIONS
	NOT INCLUDED
☐  Drywall repair, texture and paint
☐  Fixture supply unless itemized
☐  Trenching, concrete cutting, landscaping
☐  Asbestos, knob-and-tube or aluminum remediation
☐  Low voltage, data and alarm work
☐  Concealed conditions found behind finishes
	PRICE ASSUMES
☐  Working access to attic, crawlspace and panel
☐  Normal business hours, no weekend work
☐  Site clear and ready on the scheduled date
☐  Existing service entrance adequate for the new load
☐  No utility line replacement required
☐  Permit issued within the normal review time



TOTALS, DEPOSIT AND APPROVAL
	Validity: this estimate expires on the date shown in the header. Panel and wire pricing is confirmed at the time of order on longer-lead work.
PAYMENT SCHEDULE
Deposit on acceptance  $ ______________
Progress payment at _______________  $ __________
Balance on completion and inspection  $ __________
Warranty on installation labor: ________ months.
	Block A subtotal                     $ ______________
Block B subtotal                     $ ______________
Block C subtotal                     $ ______________
Labor                                     $ ______________
Materials and allowances     $ ______________
Permits at cost                      $ ______________
Tax                                          $ ______________
ESTIMATE TOTAL                $ ______________



Accepted. The scope, exclusions and assumptions above are agreed, and work beyond them is quoted separately before it starts.
	CUSTOMER SIGNATURE
	DATE

	CONTRACTOR SIGNATURE
	DATE




How to use this estimate
Delete this page, and the two lettered blocks the job does not need, before sending.
One block per job: A service call goes out on block A alone and should be one page. A panel upgrade uses block B. A rewire uses block C and usually runs longest. Combining blocks is for jobs that genuinely cover two scopes, such as a panel change during a rewire.
Site conditions first: Fill the site conditions at the walkthrough, not afterward. Existing service size, panel make, wiring age and access decide most of the price, and a quote given over the phone without them is a guess.
Permits at cost: List the fee, name the authority, and say who pulls the permit. Check the current fee schedule for the jurisdiction rather than carrying a figure forward from the last job.
Allowances: Set each allowance at a realistic middle grade, state the amount, and keep the reconciliation sentence. An allowance written without it is read as a fixed cap.
Outage window: For a panel job, write the expected hours without power on the face of the estimate. It is the detail customers remember, and the complaint it prevents costs nothing to avoid.
Exclusions: Leave the standard exclusions checked unless the job actually includes that work. Removing a line is a decision; forgetting one is a change order argument.
Validity: Keep the expiration date short enough that copper and panel pricing still holds. Reissue rather than honoring a stale number.
After acceptance: Keep the signed estimate as the source for the invoice so the quoted figure and the billed figure match, and keep the permit, the inspection result and the site photos on the same job record.

	EXAMPLE LINES, FOR REFERENCE ONLY. DELETE BEFORE USE.
Block B: existing 100 A, new 200 A, 40-space panel, meter base replaced, mast reused, four AFCI dual-function breakers added, utility disconnect requested by contractor, expected power-off window six hours.
Allowance: dining room fixture, $250 held, difference billed or credited at cost on selection.



