TREE SERVICE ESTIMATE
[Business name]   |   [Address]   |   [Phone]   |   [Email]   |   [Certified arborist credential, where held]
Replace every bracketed field, delete the gray example rows and these notes before sending. Have an attorney licensed in your state review the terms before putting this on live work, since contract and disclosure requirements vary by state.
	ESTIMATE AND PROPERTY



Estimate number  ____________________        Date  ____________________        Valid until  ____________________
Customer  ______________________________________        Phone  ____________________
Property address  ______________________________________________________________
Email  ____________________________        Walkthrough date  ____________________
Property type:  □ Residential   □ Commercial   □ HOA or association   □ Municipal
	SITE ASSESSMENT   •   completed on site before pricing


The site decides the price more than the tree does. Record it before quoting anything.
	Factor
	Finding
	Factor
	Finding

	Gate or driveway width
	______ ft
	Overhead utility lines
	yes / no, distance

	Equipment access to drop zone
	full / partial / none
	Service drop to house
	yes / no

	Drop zone available
	clear / tight / none
	Structures within fall radius
	

	Ground conditions
	firm / soft / irrigated / septic
	Slope
	

	Fence, pool or hardscape at risk
	
	Neighbor property involved
	yes / no

	Street or sidewalk closure needed
	yes / no
	Permit or protected species
	yes / no

	Photos taken and numbered
	yes / no
	Utility locate required
	yes / no


Access notes  __________________________________________________________________


TREE INVENTORY
One row per tree. Tag each tree on site with the same number that appears here, so nobody cuts the wrong one. DBH is diameter at breast height.
	Tag
	Species
	DBH in
	Height ft
	Location on lot
	Condition
	Work type
	Price

	01
	silver maple
	28
	65
	rear, near fence
	dead leader, cavity
	removal + stump
	2,850.00

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	Inventory subtotal
	$


Work type key:  REM = removal   •   TRM = trimming or pruning   •   STG = stump grinding   •   CAB = cabling or bracing   •   EMG = emergency response
Condition key:  dead   •   declining   •   structural defect   •   storm damage   •   crowding structure   •   healthy, client request
	RISK FACTORS PRICED INTO THE TREES ABOVE


□  Proximity to a structure, pool, fence or hardscape requiring rigging rather than felling
□  Overhead utility lines requiring a utility drop or standby
□  No equipment access, requiring the work to be carried out by climb and hand carry
□  Soft, irrigated or septic ground limiting machine placement
□  Dead or decayed wood making the tree unsafe to climb, requiring a crane or lift
□  Protected species, heritage tree or permit condition affecting method
□  Other: ______________________________________________


WORK DETAIL BY TYPE
	REMOVALS

	Tag
	Scope of removal
	Method
	Wood and debris
	Amount

	01
	remove to ground level, cut flush
	rigging, no crane
	haul all, chip brush
	2,400.00

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	Removals subtotal
	$

	TRIMMING AND PRUNING


Name the pruning type. "Trim the tree" is not a scope, and two crews will read it two different ways.
	Tag
	Pruning type
	Specification
	Clearance target
	Amount

	04
	crown clean and raise
	remove dead over 1 in, raise to 14 ft
	driveway clearance
	620.00

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	Trimming subtotal
	$


Pruning types quoted:  □ Crown clean   □ Crown thin   □ Crown raise   □ Crown reduction   □ Deadwood only   □ Structural or restoration   □ Clearance from structure or line
	STUMP GRINDING

	Tag
	Stump diameter
	Grind depth
	Surface roots
	Grindings
	Amount

	01
	30 in
	8 in below grade
	within 4 ft
	leave on site
	340.00

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	Stump subtotal
	$


Grindings:  □ Left on site as mulch   □ Removed and hauled   □ Backfilled with soil, no seeding   □ Backfilled and seeded
Utility locate must be completed before grinding. Irrigation lines, invisible fencing and low voltage wiring are not covered by a public locate and are the customer’s responsibility to mark.


EQUIPMENT, PERMITS AND DEBRIS
	EQUIPMENT AND ACCESS CHARGES

	Item
	Basis
	Amount

	Crane and certified operator
	day / half day
	$

	Bucket truck or lift
	day / half day
	$

	Mats or plywood for lawn and driveway protection
	per job
	$

	Additional dump trips beyond the first
	per trip
	$

	Traffic control, flagging or lane closure
	per day
	$

	Standby for utility line drop
	per occurrence
	$

	PERMITS AND APPROVALS


Permit required:  □ No   □ Yes, issued by ____________________        Fee at cost  $ ____________
Protected, heritage or ordinance-listed tree:  □ No   □ Yes, conditions: ____________________
HOA or association approval required:  □ No   □ Yes, obtained by  □ customer  □ contractor
Mitigation or replanting required by the permit:  □ No   □ Yes, priced separately
Work does not begin until any required permit and utility locate are complete.
	WOOD, BRUSH AND CLEANUP

	Material
	Disposition
	Amount

	Brush and small limbs
	chipped and hauled / chips left
	$

	Logs and large wood
	hauled / cut to length and left / split
	$

	Stump grindings
	hauled / left / backfilled
	$

	Site cleanup
	rake and blow / leave as cut
	$

	NOT INCLUDED IN THIS ESTIMATE


□  Repair of lawn, irrigation, hardscape or septic damage from necessary equipment access
□  Root pruning, root barrier installation or foundation work
□  Fence removal and reinstallation
□  Replanting, soil restoration, grading or seeding unless listed above
□  Work on neighboring property or on trees not tagged in the inventory
□  Emergency or after-hours response, which is quoted separately
□  Other: ______________________________________________


INSURANCE, TOTALS AND APPROVAL
	PROOF OF INSURANCE


Put this on the estimate rather than waiting to be asked. It is the single strongest differentiator against an uninsured bidder.
	Coverage
	Carrier
	Limit and expiration

	General liability
	
	

	Workers compensation
	
	

	Commercial auto
	
	

	Umbrella or excess, if carried
	
	


A certificate of insurance naming the customer as certificate holder is available on request and will be provided before work begins.
Credentials:  □ ISA Certified Arborist, number ____________   □ TCIA accredited   □ State license, number ____________   □ Other: ____________
	TOTALS

	
	
	Amount

	Removals
	
	$

	Trimming and pruning
	
	$

	Stump grinding
	
	$

	Equipment and access charges
	
	$

	Permits, at cost
	
	$

	Wood, brush and cleanup
	
	$

	Subtotal
	
	$

	Sales tax, where applicable
	
	$

	TOTAL ESTIMATE
	
	$

	Deposit due on approval
	
	$

	Balance due on completion
	
	$

	APPROVAL ON SITE


Trees approved for work:  □ All tagged above   □ Tags only: ____________________
Approved total  $ ______________        Deposit paid  $ ______________        Method  ____________
Scheduled date  ____________________        Expected duration  ____________________
Weather and crew scheduling may move the date. The customer is notified the same day where that happens.
Customer signature  ______________________________   Printed name  ____________________   Date  __________
Estimator signature  ______________________________   Printed name  ____________________   Date  __________
	CHANGE ORDER


Change order number  ____________    Date  ____________    Estimate number  ____________
Tree tag affected  ____________        Condition found or change requested  ____________________
Photographs numbered  ____________________
Price change  [add / deduct] $ ____________        Revised total  $ ____________
Customer approval  ______________________________   Date  __________
Contractor  _____________________________________   Date  __________
